*Installation of an mvBase Pick Patch Set*

To determine the current operating system revision, log on to SYSPROG and type **WHICH**. For systems running mvBase 2.1, these lines are returned:

RDC mvBase RELEASE 2.1

RDC mvBase BUILD 0089 where RDC is the OEM – At SAIG this is TigerLogic

*Installing mvBase Patch Sets*

**To install this patch set on the mvBase Server:**

1. Ensure all users are logged off the system.
2. **WARNING— • It is strongly recommended that you perform a VERIFY-SYSTEM and resolve any mismatches listed prior to applying this patch set. Any outstanding mismatches will cause the Patch Set installation to fail.**
   1. **• This patch set requires a *new authorization code*. We recommend that you obtain the new authorization code before applying the patch. The new code must be applied after the patch has been extracted, because the server will not start without the new code. The software serial number for obtaining the authorization code is 11031318.**
   2. **• Once this patch is successfully applied, the system is shutdown.**
   3. **NOTE—** This patch set ***must*** be installed on all computers where any mvBase component, including the mvBase Workstation or mvTerm, has been installed by the standard mvBase Setup program.
   4. This patch set contains several Windows-level mvBase components.Installation 2 mvBase 2.1 Patch Set 2 2.
   5. Perform a TLOG-CLEAR. Note that this will return the workspace and discard any transactions that have not been dequeued.
3. 3. Perform a FILE-SAVE.
4. 4. Shut down the mvBase Server, Workstation, and all instances of mvTerm on the system and close all mvBase related windows.
5. 5. Make a copy of the entire mvBase Installation file—excluding the mvBase database files (.VMS files) if the files were stored there.
6. 6. Place the self-extracting .exe file in the mvBase installation folder.
7. 7. Double-click the self-extracting .exe file, then click OK.
8. 8. Click Unzip to unzip the patch set files to the mvBase Installation folder, then click OK.
9. 9. Open the Administration Utility and apply the new authorization code.
10. 10. Restart the mvBase server and workstation.
11. 11. Log on to the SYSPROG account.
12. 12. Type: **T-SELECT *’n’* SET-TAPEFILE <mv.BASE Installation Directory>\PATCH.VTF T-ONLINE T-LOAD DICT SYSPROG-BP (0 RUN SYSPROG-BP PATCH** where *’n’* is an available Logical Tape Unit Number.
13. 13. Once the patch is successfully applied, the system is shutdown.
14. 14. Coldstart the system to resume normal operation.
15. The self-extracting .exe, .vtf, and .pdf files generated by the Patch Sets can now be removed from the mvBase Installation folder.

**To install this patch set on the mvBase Workstation:**

1. Shut down the mvBase Workstation, all instances of mvTerm on the system, and close all mvBase related windows.

2. Make a copy of the entire mvBase file.

3. Place the self extracting .exe file in the mvBase installation folder.mvBase 2.1 Patch Set 2 3

4. Double-click the self extracting .exe file, then click OK.

5. Click Unzip to unzip the patch set files to the mvBase Installation directory, then click OK.

The patch set is now installed and you can resume operations. The self-extracting .exe, .vtf, and .pdf files generated by the Patch Sets can now be removed from the mvBase Installation folder.